[PAGE_STATUS]
PAGE_STATUS.1000 =	" "
PAGE_STATUS.1001 =	" Press the Start/Stop button."
PAGE_STATUS.1002 =	" Please wait."
PAGE_STATUS.1003 =	" Please wait."
PAGE_STATUS.1004 =	" Please wait."
PAGE_STATUS.1005 =	" Please wait. Do not turn off the power while writing."
PAGE_STATUS.1006 =	" Please wait."
PAGE_STATUS.1007 =	" This mode is canceled automatically when printing is performed."
PAGE_STATUS.1008 =	" Please wait."
PAGE_STATUS.1009 =	" Please wait."
PAGE_STATUS.1010 =	" Please wait."
PAGE_STATUS.1011 =	
PAGE_STATUS.1012 =	" Please wait."
PAGE_STATUS.1013 =	" Feed paper manually, then press the Start/Stop button to start printing."
PAGE_STATUS.1014 =	" Please wait."
PAGE_STATUS.1015 =	
PAGE_STATUS.1016 =	" Please wait."
PAGE_STATUS.1017 =	
PAGE_STATUS.1018 =	
PAGE_STATUS.1019 =	" Please wait."
PAGE_STATUS.1020 =	" Check the printed results. To print the other side, remove the paper from the output tray and load it into the MP tray printed-side up so that the edge that was farthest from the paper output is fed first. Press the Start/Stop button to resume printing."
PAGE_STATUS.1021 =	" Please wait. Do not turn off the power while toner is being filled."
PAGE_STATUS.1022 =	
PAGE_STATUS.2000 =	" Turn off the printer and check the ROM module. See your reference manual for solutions."
PAGE_STATUS.2001 =	" If the quality of the print result decreases, replace the following imaging cartridges: Black(K)."
PAGE_STATUS.2002 =	" For instructions, see Help on the control panel."
PAGE_STATUS.2003 =	" For instructions, see Help on the control panel. To cancel the print job, use your computer to delete it from the print queue."
PAGE_STATUS.2004 =	" Select the correct size paper. For instructions, see Help on the control panel."
PAGE_STATUS.2005 =	
PAGE_STATUS.2006 =	
PAGE_STATUS.2007 =	
PAGE_STATUS.2008 =	" The media loaded in the printer does not match the paper type setting in the printer driver. Media that matches only the paper size setting will be used for printing. For instructions, see Help on the control panel."
PAGE_STATUS.2009 =	" Paper of the selected size or type cannot be output to the Stacker. Use the control panel to clear this warning."
PAGE_STATUS.2010 =	" Prepare a new photoconductor unit. Select Clear Warning on the control panel's Reset Menu to clear this warning."
PAGE_STATUS.2011 =	
PAGE_STATUS.2012 =	
PAGE_STATUS.2013 =	" For instructions, see Help on the control panel."
PAGE_STATUS.2014 =	
PAGE_STATUS.2015 =	
PAGE_STATUS.2016 =	
PAGE_STATUS.2017 =	" If the quality of the print result decreases, replace the following imaging cartridges: Black(K)."
PAGE_STATUS.2018 =	" If the quality of the print result decreases, replace the following imaging cartridges: Cyan(C)."
PAGE_STATUS.2019 =	" If the quality of the print result decreases, replace the following imaging cartridges: Black(K), Cyan(C)."
PAGE_STATUS.2020 =	" If the quality of the print result decreases, replace the following imaging cartridges: Magenta(M)."
PAGE_STATUS.2021 =	" If the quality of the print result decreases, replace the following imaging cartridges: Black(K), Magenta(M)."
PAGE_STATUS.2022 =	" If the quality of the print result decreases, replace the following imaging cartridges: Cyan(C), Magenta(M)."
PAGE_STATUS.2023 =	" If the quality of the print result decreases, replace the following imaging cartridges: Black(K), Cyan(C), Magenta(M)."
PAGE_STATUS.2024 =	" If the quality of the print result decreases, replace the following imaging cartridges: Yellow(Y)."
PAGE_STATUS.2025 =	" If the quality of the print result decreases, replace the following imaging cartridges: Black(K), Yellow(Y)."
PAGE_STATUS.2026 =	" If the quality of the print result decreases, replace the following imaging cartridges: Cyan(C), Yellow(Y)."
PAGE_STATUS.2027 =	" If the quality of the print result decreases, replace the following imaging cartridges: Black(K), Cyan(C), Yellow(Y)."
PAGE_STATUS.2028 =	" If the quality of the print result decreases, replace the following imaging cartridges: Magenta(M), Yellow(Y)."
PAGE_STATUS.2029 =	" If the quality of the print result decreases, replace the following imaging cartridges: Black(K), Magenta(M), Yellow(Y)."
PAGE_STATUS.2030 =	" If the quality of the print result decreases, replace the following imaging cartridges: Cyan(C), Magenta(M), Yellow(Y)."
PAGE_STATUS.2031 =	" If the quality of the print result decreases, replace the following imaging cartridges: Black(K), Cyan(C), Magenta(M), Yellow(Y)."
PAGE_STATUS.2049 =	
PAGE_STATUS.2050 =	
PAGE_STATUS.2051 =	
PAGE_STATUS.2052 =	
PAGE_STATUS.2053 =	
PAGE_STATUS.2054 =	
PAGE_STATUS.2055 =	
PAGE_STATUS.2056 =	
PAGE_STATUS.2057 =	
PAGE_STATUS.2058 =	
PAGE_STATUS.2059 =	
PAGE_STATUS.2060 =	
PAGE_STATUS.2061 =	
PAGE_STATUS.2062 =	
PAGE_STATUS.2063 =	
PAGE_STATUS.2065 =	" Clean the following parts:Cleaning knob a."
PAGE_STATUS.2066 =	" Clean the following parts:Cleaning knob b."
PAGE_STATUS.2067 =	" Clean the following parts:Cleaning knob a and b."
PAGE_STATUS.2068 =	" Clean the following parts:Cleaning knob."
PAGE_STATUS.2069 =	" Clean the following parts:Cleaning knob a."
PAGE_STATUS.2070 =	" Clean the following parts:Cleaning knob b."
PAGE_STATUS.2071 =	" Clean the following parts:Cleaning knob a and b."
PAGE_STATUS.2072 =	" Select the correct printer driver. Use the control panel to clear this warning."
PAGE_STATUS.2073 =	" Remove the incorrect USB device. Use the control panel to clear this warning.   Reset Menu > Clear Warning "
PAGE_STATUS.2074 =	" Use the control panel to clear this warning.   Reset Menu > Clear Warning "
PAGE_STATUS.2560 =	
PAGE_STATUS.2561 =	" There is not enough space on the printer's hard disk to install all of the PostScript fonts. Uninstall some existing fonts. Use the control panel to clear this warning."
PAGE_STATUS.2562 =	" Replace with a new fuser unit. Select Clear Warning on the control panel's Reset Menu to clear this message."
PAGE_STATUS.2563 =	" Prepare a new transfer unit. Select Clear Warning on the control panel's Reset Menu to clear this message."
PAGE_STATUS.2564 =	
PAGE_STATUS.2565 =	" For instructions, see Help on the control panel or press the Information button."
PAGE_STATUS.2566 =	
PAGE_STATUS.2567 =	" Upgrade to the latest printer driver. If this warning appears again, contact your dealer. Select Clear Warning on the control panel's Reset Menu to clear this warning."
PAGE_STATUS.2568 =	
PAGE_STATUS.2569 =	" There is not enough space on the printer's hard disk. Delete unnecessary data from the printer's hard disk. Use the control panel to clear this warning."
PAGE_STATUS.2570 =	" There is not enough space on the printer's hard disk or the maximum number of form data files that can be stored on the disk has been reached. Delete unnecessary data from the printer's hard disk. Use the control panel to clear this warning."
PAGE_STATUS.2571 =	" The following consumables are near the end of their service life."
PAGE_STATUS.3000 =	" Press the Start/Stop button to print again. Press the Cancel Job button to cancel the print job. Use the control panel so that this error may be avoided. Setup Menu > Page Protect > On If this error occurs again, add printer memory."
PAGE_STATUS.3001 =	" For instructions, see Help on the control panel."
PAGE_STATUS.3002 =	
PAGE_STATUS.3003 =	" For instructions, see Help on the control panel."
PAGE_STATUS.3004 =	" For instructions, see Help on the control panel."
PAGE_STATUS.3005 =	" For instructions, see Help on the control panel."
PAGE_STATUS.3006 =	" Set the paper path selector on the printer to the position for face-down output. Press the Start/Stop button to resume printing."
PAGE_STATUS.3007 =	" Cancel all print jobs remaining on your computer and check all cable connections. Then, press the Cancel Job button for a few seconds to cancel all print jobs on the printer."
PAGE_STATUS.3008 =	" For instructions, see Help on the control panel."
PAGE_STATUS.4000 =	" Open the top cover, then install the imaging cartridge."
PAGE_STATUS.4001 =	" Open the top cover, then replace the imaging cartridge."
PAGE_STATUS.4002 =	" Close the cover."
PAGE_STATUS.4003 =	" Turn off the printer and replace the ROM module."
PAGE_STATUS.4004 =	
PAGE_STATUS.4005 =	
PAGE_STATUS.4006 =	" Turn off the printer and check the ROM module."
PAGE_STATUS.4007 =	" Install the cassette."
PAGE_STATUS.4008 =	" Open the top cover and remove any jammed paper."
PAGE_STATUS.4009 =	" Remove any jammed paper from the MP tray or paper cassette. Reload the paper, then open and close the top cover. Printing will resume from the page that jammed."
PAGE_STATUS.4010 =	" Load the paper."
PAGE_STATUS.4011 =	
PAGE_STATUS.4012 =	" Open the top cover and remove any jammed paper."
PAGE_STATUS.4013 =	" The interface card installed is incompatible or defective. Turn off the printer. Remove the interface card, then turn the printer back on. If this error occurs again, contact your dealer."
PAGE_STATUS.4014 =	" The interface card installed is incompatible or defective. Turn off the printer. Remove the interface card, then turn the printer back on. If this error occurs again, contact your dealer."
PAGE_STATUS.4015 =	" Close the cover."
PAGE_STATUS.4016 =	" Remove any jammed paper and load paper of the correct size. Printing will resume at the current page. For instructions, see Help on the control panel. "
PAGE_STATUS.4017 =	" Open the Duplex Unit and remove any jammed paper."
PAGE_STATUS.4018 =	
PAGE_STATUS.4019 =	
PAGE_STATUS.4020 =	
PAGE_STATUS.4021 =	" The media loaded in the printer does not match the paper type selected in the printer driver. For instructions, see Help on the control panel. "
PAGE_STATUS.4022 =	" Open covers A and D, then install the photoconductor unit correctly."
PAGE_STATUS.4023 =	
PAGE_STATUS.4024 =	
PAGE_STATUS.4025 =	
PAGE_STATUS.4026 =	
PAGE_STATUS.4027 =	
PAGE_STATUS.4028 =	" Open covers A and D, then replace the photoconductor unit."
PAGE_STATUS.4029 =	
PAGE_STATUS.4030 =	
PAGE_STATUS.4031 =	" Cancel all print jobs remaining on your computer. Open cover E and remove any jammed paper. If the optional Duplex Unit is installed, open cover D first, then open cover E and remove any jammed paper. Turn off the printer. Wait a few minutes, then turn the printer back on. This error may be avoided by reducing the color density of your document."
PAGE_STATUS.4032 =	" Open covers A and D, then install a compatible photoconductor unit."
PAGE_STATUS.4033 =	
PAGE_STATUS.4034 =	
PAGE_STATUS.4035 =	
PAGE_STATUS.4036 =	
PAGE_STATUS.4037 =	
PAGE_STATUS.4038 =	" Close the cover."
PAGE_STATUS.4039 =	
PAGE_STATUS.4040 =	
PAGE_STATUS.4041 =	
PAGE_STATUS.4042 =	
PAGE_STATUS.4045 =	" Install the unit correctly."
PAGE_STATUS.4046 =	
PAGE_STATUS.4047 =	
PAGE_STATUS.4048 =	
PAGE_STATUS.4049 =	" Open the top cover and install the following toner cartridges correctly: Black(K)."
PAGE_STATUS.4050 =	" Open the top cover and install the following toner cartridges correctly: Cyan(C)."
PAGE_STATUS.4051 =	" Open the top cover and install the following toner cartridges correctly: Black(K), Cyan(C)."
PAGE_STATUS.4052 =	" Open the top cover and install the following toner cartridges correctly: Magenta(M)."
PAGE_STATUS.4053 =	" Open the top cover and install the following toner cartridges correctly: Black(K), Magenta(M)."
PAGE_STATUS.4054 =	" Open the top cover and install the following toner cartridges correctly: Cyan(C), Magenta(M)."
PAGE_STATUS.4055 =	" Open the top cover and install the following toner cartridges correctly: Black(K), Cyan(C), Magenta(M)."
PAGE_STATUS.4056 =	" Open the top cover and install the following toner cartridges correctly: Yellow(Y)."
PAGE_STATUS.4057 =	" Open the top cover and install the following toner cartridges correctly: Black(K), Yellow(Y)."
PAGE_STATUS.4058 =	" Open the top cover and install the following toner cartridges correctly: Cyan(C), Yellow(Y)."
PAGE_STATUS.4059 =	" Open the top cover and install the following toner cartridges correctly: Black(K), Cyan(C), Yellow(Y)."
PAGE_STATUS.4060 =	" Open the top cover and install the following toner cartridges correctly: Magenta(M), Yellow(Y)."
PAGE_STATUS.4061 =	" Open the top cover and install the following toner cartridges correctly: Black(K), Magenta(M), Yellow(Y)."
PAGE_STATUS.4062 =	" Open the top cover and install the following toner cartridges correctly: Cyan(C), Magenta(M), Yellow(Y)."
PAGE_STATUS.4063 =	" Open the top cover and install the following toner cartridges correctly: Black(K), Cyan(C), Magenta(M), Yellow(Y)."
PAGE_STATUS.4065 =	" Open the top cover and replace the following toner cartridges: Black(K)."
PAGE_STATUS.4066 =	" Open the top cover and replace the following toner cartridges: Cyan(C)."
PAGE_STATUS.4067 =	" Open the top cover and replace the following toner cartridges: Black(K), Cyan(C)."
PAGE_STATUS.4068 =	" Open the top cover and replace the following toner cartridges: Magenta(M)."
PAGE_STATUS.4069 =	" Open the top cover and replace the following toner cartridges: Black(K), Magenta(M)."
PAGE_STATUS.4070 =	" Open the top cover and replace the following toner cartridges: Cyan(C), Magenta(M)."
PAGE_STATUS.4071 =	" Open the top cover and replace the following toner cartridges: Black(K), Cyan(C), Magenta(M)."
PAGE_STATUS.4072 =	" Open the top cover and replace the following toner cartridges: Yellow(Y)."
PAGE_STATUS.4073 =	" Open the top cover and replace the following toner cartridges: Black(K), Yellow(Y)."
PAGE_STATUS.4074 =	" Open the top cover and replace the following toner cartridges: Cyan(C), Yellow(Y)."
PAGE_STATUS.4075 =	" Open the top cover and replace the following toner cartridges: Black(K), Cyan(C), Yellow(Y)."
PAGE_STATUS.4076 =	" Open the top cover and replace the following toner cartridges: Magenta(M), Yellow(Y)."
PAGE_STATUS.4077 =	" Open the top cover and replace the following toner cartridges: Black(K), Magenta(M), Yellow(Y)."
PAGE_STATUS.4078 =	" Open the top cover and replace the following toner cartridges: Cyan(C), Magenta(M), Yellow(Y)."
PAGE_STATUS.4079 =	" Open the top cover and replace the following toner cartridges: Black(K), Cyan(C), Magenta(M), Yellow(Y)."
PAGE_STATUS.4080 =	
PAGE_STATUS.4081 =	
PAGE_STATUS.4082 =	
PAGE_STATUS.4083 =	
PAGE_STATUS.4084 =	" Open the top cover, then remove and reinstall the imaging cartridge. If this error occurs again, replace the imaging cartridge."
PAGE_STATUS.4085 =	" Open the top cover and reinstall or replace the imaging cartridge."
PAGE_STATUS.4086 =	
PAGE_STATUS.4087 =	
PAGE_STATUS.4088 =	
PAGE_STATUS.4089 =	
PAGE_STATUS.4090 =	" Remove the paper from the tray. Press the Start/Stop button to resume printing."
PAGE_STATUS.4091 =	
PAGE_STATUS.4092 =	
PAGE_STATUS.4093 =	
PAGE_STATUS.4094 =	
PAGE_STATUS.4095 =	
PAGE_STATUS.4096 =	
PAGE_STATUS.4097 =	
PAGE_STATUS.4098 =	
PAGE_STATUS.4099 =	
PAGE_STATUS.4100 =	
PAGE_STATUS.4101 =	" Remove the paper from the bin and press the Start/Stop button to resume printing."
PAGE_STATUS.4102 =	" Remove the paper from the bin and press the Start/Stop button to resume printing."
PAGE_STATUS.4103 =	" Remove the paper from the bin and press the Start/Stop button to resume printing."
PAGE_STATUS.4104 =	" Remove the paper from the bin and press the Start/Stop button to resume printing."
PAGE_STATUS.4105 =	" Remove the paper from the bin and press the Start/Stop button to resume printing."
PAGE_STATUS.4106 =	" Remove the paper from the bin and press the Start/Stop button to resume printing."
PAGE_STATUS.4107 =	" Remove the paper from the bin and press the Start/Stop button to resume printing."
PAGE_STATUS.4108 =	" Remove the paper from the bin and press the Start/Stop button to resume printing."
PAGE_STATUS.4109 =	" Remove the paper from the bin and press the Start/Stop button to resume printing."
PAGE_STATUS.4200 =	
PAGE_STATUS.4201 =	" Contact your dealer."
PAGE_STATUS.4202 =	" Turn off the printer, then reinstall or remove the hard disk."
PAGE_STATUS.4203 =	
PAGE_STATUS.4204 =	
PAGE_STATUS.4205 =	" Open the Mailbox unit cover and remove any jammed paper."
PAGE_STATUS.4206 =	
PAGE_STATUS.4207 =	" Remove the paper from the tray. Press the Start/Stop button to resume printing."
PAGE_STATUS.4208 =	
PAGE_STATUS.4209 =	
PAGE_STATUS.4210 =	
PAGE_STATUS.4211 =	
PAGE_STATUS.4212 =	
PAGE_STATUS.4213 =	
PAGE_STATUS.4214 =	
PAGE_STATUS.4215 =	
PAGE_STATUS.4216 =	
PAGE_STATUS.4217 =	
PAGE_STATUS.4218 =	
PAGE_STATUS.4221 =	" Turn off the printer. Open covers A and D, then close A and open B. Install the fuser unit correctly. If this error occurs again, replace with a new fuser unit."
PAGE_STATUS.4222 =	" Open cover A, then install the transfer unit correctly."
PAGE_STATUS.4223 =	
PAGE_STATUS.4224 =	" Open cover A, then replace the transfer unit."
PAGE_STATUS.4225 =	
PAGE_STATUS.4226 =	" The media loaded in the printer does not match the paper type selected in the printer driver. Press the Start/Stop button to resume printing. Press the Cancel Job button to cancel the print job."
PAGE_STATUS.4227 =	
PAGE_STATUS.4228 =	" For instructions, see Help on the control panel."
PAGE_STATUS.4229 =	" Load the correct size paper. Press the Start/Stop button to resume printing."
PAGE_STATUS.4230 =	" Open the top cover, then replace the imaging cartridge."
PAGE_STATUS.4231 =	" Remove all installed paper cassettes, then gently remove any paper that has been fed part way into the printer."
PAGE_STATUS.4232 =	" Turn off the printer and replace the IPDS module."
PAGE_STATUS.4233 =	
PAGE_STATUS.4234 =	" Paper is jammed in one of the following locations:  Cover DM   MP Tray  Cassette 1  Cassette 2  Cassette 3  Cover A  Cover B  Cover STK For instructions, see Help on the control panel."
PAGE_STATUS.4235 =	" Install the toner cartridge correctly."
PAGE_STATUS.4236 =	" Replace the following:  Fuser unit  Maintenance unit  Feed roller C2  Feed roller C3  Toner cartridge For instructions, see Help on the control panel."
PAGE_STATUS.4237 =	" Replace the toner cartridge."
PAGE_STATUS.4238 =	" Replace the toner cartridge."
PAGE_STATUS.4239 =	" Close the following covers:  Cover A or B  Cover DM  Cover STK"
PAGE_STATUS.4240 =	" Contact your dealer."
PAGE_STATUS.4241 =	" The installed toner cartridge differs from the genuine EPSON toner cartridge for this printer. For instructions, see the control panel. Black(K)."
PAGE_STATUS.4242 =	" The installed toner cartridge differs from the genuine EPSON toner cartridge for this printer. For instructions, see the control panel. Cyan(C)."
PAGE_STATUS.4243 =	" The installed toner cartridge differs from the genuine EPSON toner cartridge for this printer. For instructions, see the control panel. Black(K), Cyan(C)."
PAGE_STATUS.4244 =	" The installed toner cartridge differs from the genuine EPSON toner cartridge for this printer. For instructions, see the control panel. Magenta(M)."
PAGE_STATUS.4245 =	" The installed toner cartridge differs from the genuine EPSON toner cartridge for this printer. For instructions, see the control panel. Black(K), Magenta(M)."
PAGE_STATUS.4246 =	" The installed toner cartridge differs from the genuine EPSON toner cartridge for this printer. For instructions, see the control panel. Cyan(C), Magenta(M)."
PAGE_STATUS.4247 =	" The installed toner cartridge differs from the genuine EPSON toner cartridge for this printer. For instructions, see the control panel. Black(K), Cyan(C), Magenta(M)."
PAGE_STATUS.4248 =	" The installed toner cartridge differs from the genuine EPSON toner cartridge for this printer. For instructions, see the control panel. Yellow(Y)."
PAGE_STATUS.4249 =	" The installed toner cartridge differs from the genuine EPSON toner cartridge for this printer. For instructions, see the control panel. Black(K), Yellow(Y)."
PAGE_STATUS.4250 =	" The installed toner cartridge differs from the genuine EPSON toner cartridge for this printer. For instructions, see the control panel. Cyan(C), Yellow(Y)."
PAGE_STATUS.4251 =	" The installed toner cartridge differs from the genuine EPSON toner cartridge for this printer. For instructions, see the control panel. Black(K), Cyan(C), Yellow(Y)."
PAGE_STATUS.4252 =	" The installed toner cartridge differs from the genuine EPSON toner cartridge for this printer. For instructions, see the control panel. Magenta(M), Yellow(Y)."
PAGE_STATUS.4253 =	" The installed toner cartridge differs from the genuine EPSON toner cartridge for this printer. For instructions, see the control panel. Black(K), Magenta(M), Yellow(Y)."
PAGE_STATUS.4254 =	" The installed toner cartridge differs from the genuine EPSON toner cartridge for this printer. For instructions, see the control panel. Cyan(C), Magenta(M), Yellow(Y)."
PAGE_STATUS.4255 =	" The installed toner cartridge differs from the genuine EPSON toner cartridge for this printer. For instructions, see the control panel. Black(K), Cyan(C), Magenta(M), Yellow(Y)."
PAGE_STATUS.4256 =	" Contact your dealer."
PAGE_STATUS.4257 =	" Open cover B, remove the photoconductor unit, and then close cover B. Toner cartridges can be installed."
PAGE_STATUS.4258 =	" Remove the toner cartridge from the installation position. For instructions, see Help on the control panel. "
PAGE_STATUS.4259 =	" Replace the toner cartridge in the installation position with a toner cartridge of the color displayed on the control panel. For instructions, see Help on the control panel."
PAGE_STATUS.4260 =	" Replace the toner cartridge in the installation position with a toner cartridge of the color displayed on the control panel. For instructions, see Help on the control panel."
PAGE_STATUS.4261 =	" Replace the toner cartridge in the installation position with a toner cartridge of the color displayed on the control panel. For instructions, see Help on the control panel."
PAGE_STATUS.4262 =	" Replace the toner cartridge in the installation position with a toner cartridge of the color displayed on the control panel. For instructions, see Help on the control panel."
PAGE_STATUS.4263 =	
PAGE_STATUS.4264 =	
PAGE_STATUS.6000 =	" Turn off the printer and make sure any optional interfaces, memory modules, or ROM modules are installed correctly. Wait a few minutes, then turn on the printer.If this error occurs again, contact your dealer."
PAGE_STATUS.6001 =	" Turn off the printer and make sure any optional interfaces, memory modules, or ROM modules are installed correctly. Wait a few minutes, then turn on the printer.If this error occurs again, contact your dealer and tell them the error number that appears."
PAGE_STATUS.40001 =	" Turn off the printer, then install the Duplex Unit and the Cassettes correctly."
PAGE_STATUS.40002 =	" Turn off the printer, then install the Duplex Unit and the Stacker correctly."
PAGE_STATUS.40003 =	" Turn off the printer, then install optional cassettes for this printer correctly."
PAGE_STATUS.UNKNOWN =	" Check the printer. To display the correct status message, it may help to install the latest EPSON Status Monitor."

[INK_STATUS]
INK_STATUS.0x00 = " "
INK_STATUS.0x01 = " "
INK_STATUS.0x02 = " Please wait."
INK_STATUS.0x03 = " Please wait."
INK_STATUS.0x04 = " "
INK_STATUS.0x05 = " Press the Pause button."
INK_STATUS.0x06 = " "
INK_STATUS.0x07 = " Please wait."
INK_STATUS.0x08 = " Set a correct ink cartridge.Use of a genuine cartridge is recommended."
INK_STATUS.0x09 = " "
INK_STATUS.0x0A = " Please wait."
INK_STATUS.0x0B = " "
INK_STATUS.UNKNOWN = ""

[INK_ERR]
INK_ERR.0x00 = " Delete all print jobs and turn the printer off. Remove any foreign objects from inside the printer. After a few minutes, turn the printer back on. If the error message still appears, contact the store where you purchased the product or an Epson service center. "
INK_ERR.0x01 = " Please wait."
INK_ERR.0x02 = " Close the cover."
INK_ERR.0x03 = 
INK_ERR.0x04 = " Remove the paper."
INK_ERR.0x05 = " Replace the ink cartridge.Use of a genuine cartridge is recommended."
INK_ERR.0x06 = " Load the paper."
INK_ERR.0x07 = 
INK_ERR.0x08 = 
INK_ERR.0x09 = " If continuous paper is currently loaded, tear off the paper at the appropriate place, then press the Pause button to eject it. Load cut-sheet paper, then press the pause button again to start printing. If cut-sheet paper is loaded, turn off the printer and remove the paper from the paper path. Load continuous paper. Cancel the print job, then turn the printer back on. Send the print job again."
INK_ERR.0x0A = " Modify the paper size on the printer driver to match the loaded paper. "
INK_ERR.0x0B = 
INK_ERR.0x0C = " Specify the correct media source."
INK_ERR.0x0D = 
INK_ERR.0x0E = 
INK_ERR.0x0F = 
INK_ERR.0x10 = " If the error message still appears, contact the store where you purchased the product or an Epson service center."
INK_ERR.0x11 = 
INK_ERR.0x12 = " A page has not been printed, multiple pages have been fed into the printer at once, or the wrong paper size has been fed into the printer. Remove and reload the paper. Press the [Paper] or [OK] button if necessary."
INK_ERR.0x13 = 
INK_ERR.0x14 = 
INK_ERR.0x15 = 
INK_ERR.0x16 = 
INK_ERR.0x17 = " Set the correct paper, or check the media layout settings or paper position detection settings. "
INK_ERR.0x18 = 
INK_ERR.0x19 = 
INK_ERR.0x1A = " Close the ink cartridge cover and move the cartridge lock lever to the lock position."
INK_ERR.0x1B = 
INK_ERR.0x1C = 
INK_ERR.0x1D = 
INK_ERR.0x1E = 
INK_ERR.0x1F = 
INK_ERR.0x20 = 
INK_ERR.0x22 = " Install the maintenance box."
INK_ERR.0x23 = 
INK_ERR.0x24 = 
INK_ERR.0x25 = " Remove any remaining paper by hand, and then set the Auto Duplexer correctly."
INK_ERR.0x26 = 
INK_ERR.0x27 = 
INK_ERR.0x28 = 
INK_ERR.0x29 = " Attach the cassette tray."
INK_ERR.0x2C = " Use of a genuine cartridge is recommended."
INK_ERR.0x36 = " Make sure the maintenance box is installed, and then close the maintenance box cover."
INK_ERR.0x37 = " Close the printer cover."
INK_ERR.0x3F = " Remove the loaded new paper once. Remove any paper which is still in the printer and load the new paper again."
INK_ERR.0x41 = " Parts inside your printer are at the end of their service life. See your printer documentation."
INK_ERR.UNKNOWN = " Turn the printer off, and remove any jammed paper. After a few minutes, turn the printer back on."

[INK_SP]
INK_SP.0x00 = " Please wait."
INK_SP.0x01 = 
INK_SP.0x02 = 
INK_SP.0x03 = " Please wait."
INK_SP.UNKNOWN = 

[INK_FATAL_ERR]
INK_FATAL_ERR.0x54.TM-C600 = " "
INK_FATAL_ERR.0x54.TM-C3400 = " "
INK_FATAL_ERR.0x7B.TM-C3400 = " Set the ambient temperature within 10ºC {50ºF} and 35ºC {95ºF}, turn off the printer and then turn it back on."
INK_FATAL_ERR.0x7C.TM-C3400 = " Set the ambient temperature within 10ºC {50ºF} and 35ºC {95ºF}, turn off the printer and then turn it back on."
INK_FATAL_ERR.UNKNOWN = " Delete all print jobs and turn the printer off. Remove any foreign objects from inside the printer. After a few minutes, turn the printer back on. If the error message still appears, contact the store where you purchased the product or an Epson service center. "

[INK_WARNING]
INK_WARNING.0x00 = 
INK_WARNING.0x01 = 
INK_WARNING.0x02 = 
INK_WARNING.0x10 = " Get a new ink cartridge ready. Use of a genuine cartridge is recommended.(%s)"
INK_WARNING.0x11 = " Get a new ink cartridge ready. Use of a genuine cartridge is recommended.(%s)"
INK_WARNING.0x12 = " Get a new ink cartridge ready. Use of a genuine cartridge is recommended.(%s)"
INK_WARNING.0x13 = " Get a new ink cartridge ready. Use of a genuine cartridge is recommended.(%s)"
INK_WARNING.0x14 = " Get a new ink cartridge ready. Use of a genuine cartridge is recommended.(%s)"
INK_WARNING.0x15 = " Get a new ink cartridge ready. Use of a genuine cartridge is recommended.(%s)"
INK_WARNING.0x16 = " Get a new ink cartridge ready. Use of a genuine cartridge is recommended.(%s)"
INK_WARNING.0x17 = " Get a new ink cartridge ready. Use of a genuine cartridge is recommended.(%s)"
INK_WARNING.0x18 = " Get a new ink cartridge ready. Use of a genuine cartridge is recommended.(%s)"
INK_WARNING.0x19 = " Get a new ink cartridge ready. Use of a genuine cartridge is recommended.(%s)"
INK_WARNING.0x1A = " Get a new ink cartridge ready. Use of a genuine cartridge is recommended.(%s)"
INK_WARNING.0x1B = " Get a new ink cartridge ready. Use of a genuine cartridge is recommended.(%s)"
INK_WARNING.0x1C = " Get a new ink cartridge ready. Use of a genuine cartridge is recommended.(%s)"
INK_WARNING.0x1D = " Get a new ink cartridge ready. Use of a genuine cartridge is recommended.(%s)"
INK_WARNING.0x1E = " Get a new ink cartridge ready. Use of a genuine cartridge is recommended.(%s)"
INK_WARNING.0x1F = " Get a new ink cartridge ready. Use of a genuine cartridge is recommended.(%s)"
INK_WARNING.0x20 = " "
INK_WARNING.0x21 = " Parts inside your printer are near the end of their service life. See your printer documentation."
INK_WARNING.0x30 = " "
INK_WARNING.0x31 = " "
INK_WARNING.0x32 = " "
INK_WARNING.0x33 = " "
INK_WARNING.0x34 = " "
INK_WARNING.0x35 = " "
INK_WARNING.0x36 = " "
INK_WARNING.0x37 = " "
INK_WARNING.0x38 = " "
INK_WARNING.0x39 = " "
INK_WARNING.0x40 = " Close the ink cover."
INK_WARNING.0x42 = " Get a new ink cartridge ready.Use of a genuine cartridge is recommended."
INK_WARNING.UNKNOWN = ""

[TM_ASB]
TM_ASB.0 = " "
TM_ASB.8 = " Prepare the paper."
TM_ASB.9 = " Prepare the paper."
TM_ASB.10 = " Replace the paper."
TM_ASB.11 = " Replace the paper."
TM_ASB.16 = " Remove the slip."
TM_ASB.18 = " Make sure that the cover is properly closed.If a paper jam has occurred, remove the jammed paper.Turn off the printer, and turn it back on after a while."
TM_ASB.19 = " "
TM_ASB.21 = " "
TM_ASB.22 = " Please wait."
TM_ASB.27 = " "
TM_ASB.29 = " Close the cover."
TM_ASB.-1 = " "
TM_ASB.UNKNOWN = ""

[TM_INKASB]
TM_INKASB.16 = " Get a new ink cartridge ready."
TM_INKASB.17 = " Replace the ink cartridge."
TM_INKASB.24 = " Get a new ink cartridge ready."
TM_INKASB.25 = " Replace the ink cartridge."
TM_INKASB.26 = " Replace the ink cartridge."
TM_INKASB.27 = " Replace the ink cartridge."
TM_INKASB.UNKNOWN = ""